DEVLINK-REGION(8)

NAME
devlink-region - devlink address region access

SYNOPSIS

devlink [ OPTIONS ] region { COMMAND | help }

OPTIONS := { -V[ersion] | -n[no-nice-names] }
devlink region show [ DEV/REGION ]
devlink region new DEV/REGION [ snapshot SNAPSHOT_ID ]
devlink region del DEV/REGION snapshot SNAPSHOT_ID
devlink region dump DEV/REGION snapshot SNAPSHOT_ID
devlink region read DEV/REGION [ snapshot SNAPSHOT_ID ] address ADDRESS length LENGTH
devlink region help

DESCRIPTION

  devlink region show - Show all supported address regions names, snapshots and sizes

DEV/REGION - specifies the devlink device and address-region to query.

  devlink region new - Create a snapshot specified by address-region name and snapshot ID

DEV/REGION - specifies the devlink device and address-region to snapshot

snapshot SNAPSHOT_ID - optionally specifies the snapshot ID to assign. If not specified, devlink will assign a unique ID to the snapshot.

  devlink region del - Delete a snapshot specified by address-region name and snapshot ID

DEV/REGION - specifies the devlink device and address-region to delete the snapshot from

snapshot SNAPSHOT_ID - specifies the snapshot ID to delete

  devlink region dump - Dump all the available data from a region or from snapshot of a region

DEV/REGION - specifies the device and address-region to dump from.

snapshot SNAPSHOT_ID - specifies the snapshot-id of the region to dump.

  devlink region read - Read from a specific region address for a given length

DEV/REGION - specifies the device and address-region to read from.

snapshot SNAPSHOT_ID - specifies the snapshot-id of the region to read.

address ADDRESS - specifies the address to read from.

length LENGTH - specifies the length of data to read.

EXAMPLES

devlink region show
    List available address regions and snapshot.

devlink region new pci/0000:00:05.0/cr-space
    Create a new snapshot from cr-space address region from device pci/0000:00:05.0.

devlink region del pci/0000:00:05.0/cr-space snapshot 1
    Delete snapshot id 1 from cr-space address region from device pci/0000:00:05.0.

devlink region dump pci/0000:00:05.0/cr-space snapshot 1
    Dump the snapshot taken from cr-space address region with ID 1

devlink region read pci/0000:00:05.0/cr-space snapshot 1 address 0x10 length 16
    Read from address 0x10, 16 Bytes of snapshot ID 1 taken from cr-space address region

SEE ALSO
devlink(8), devlink-dev(8), devlink-port(8), devlink-monitor(8),

AUTHOR
Alex Vesker <valex@mellanox.com>