DEVLINK-LC(8)

NAME
devlink-lc - devlink line card configuration

SYNOPSIS

devlink [ OPTIONS ] lc { COMMAND | help }

OPTIONS := { -V[ersion] }
devlink lc set DEV lc LC_INDEX [ type { LC_TYPE | notype } ]
devlink lc show [ DEV [ lc LC_INDEX ] ]
devlink lc help

DESCRIPTION

  devlink lc set - change line card attributes

DEV Specifies the devlink device to operate on.
    Format is:
    BUS_NAME/BUS_ADDRESS

lc LC_INDEX
    Specifies index of a line card slot to set.

type {
    LC_TYPE | notype } Type of line card to provision. Each driver provides a list of supported line card types which is shown in the output of devlink lc show command.

  devlink lc show - display line card attributes

DEV Specifies the devlink device to operate on. If this and lc arguments are omitted all line cards of all devices are listed.

lc LC_INDEX
    Specifies index of a line card slot to show.

EXAMPLES

devlink lc show
    Shows the state of all line cards on the system.

devlink lc show pci/0000:01:00.0 lc 1
    Shows the state of line card with index 1.

devlink lc set pci/0000:01:00.0 lc 1 type 16x100G
    Sets type of specified line card to type 16x100G.

devlink lc set pci/0000:01:00.0 lc 1 notype
    Clears provisioning on a line card.

SEE ALSO
devlink(8), devlink-dev(8), devlink-port(8), devlink-monitor(8),

AUTHOR
Jiri Pirko <jiri@nvidia.com>