Generic packet editor action in tc(8)

NAME
pedit - generic packet editor action

SYNOPSIS
tc ... action pedit [ex] munge { RAW_OP | LAYERED_OP | EXTENDED_LAYERED_OP } [ CONTROL ]
RAW_OP := offset OFFSET { u8 | u16 | u32 } [ AT_SPEC ] CMD_SPEC
AT_SPEC := at AT offmask MASK shift SHIFT
LAYERED_OP := { ip IPHDR_FIELD | ip BEYOND_IPHDR_FIELD } CMD_SPEC
EXTENDED_LAYERED_OP := { eth ETHHDR_FIELD | ip IPHDR_FIELD | ip EX_IPHDR_FIELD | ip6 IP6HDR_FIELD | tcp TCPHDR_FIELD | udp UDPHDR_FIELD } CMD_SPEC
ETHHDR_FIELD := { src | dst | type }
IPHDR_FIELD := { src | dst | tos | dsfield | ihl | protocol | precedence | nofrag | firstfrag | ce | df }
BEYOND_IPHDR_FIELD := { dport | sport | icmp_type | icmp_code }
EX_IPHDR_FIELD := { ttl }
IP6HDR_FIELD := { src | dst | traffic_class | flow_lbl | payload_len | nexthdr | hoplimit }
TCPHDR_FIELD := { sport | dport | flags }
UDPHDR_FIELD := { sport | dport }
CMD_SPEC := { clear | invert | set VAL | add VAL | decrement | preserve } [ retain RVAL ]
CONTROL := { reclassify | pipe | drop | shot | continue | pass | goto chain CHAIN_INDEX }

DESCRIPTION
The pedit action can be used to change arbitrary packet data. The location of data to change can either be specified by giving an offset and size as in RAW_OP, or for header values by naming the header and field to edit the size is then chosen automatically based on the header field size.

OPTIONS

ex  Use extended pedit. EXTENDED_LAYERED_OP and the add/decrement CMD_SPEC are allowed only in this mode.

offset OFFSET { u32 | u16 | u8 }
    Specify the offset at which to change data. OFFSET is a signed integer, it's base is automatically chosen (e.g. hex if prefixed by 0x or octal if prefixed by 0). The second argument specifies the length of data to change, that is four bytes (u32), two bytes (u16) or a single byte (u8).

at AT offmask MASK shift SHIFT
    This is an optional part of RAW_OP which allows one to have a variable OFFSET depending on packet data at offset AT, which is binary ANDed with MASK and right-shifted by SHIFT before adding it to OFFSET.

eth ETHHDR_FIELD
    Change an ETH header field. The supported keywords for ETHHDR_FIELD are:

    src
    dst
        Source or destination MAC address in the standard format: XX:XX:XX:XX:XX:XX

    type
        Ether-type in numeric value

ip IPHDR_FIELD
    Change an IPv4 header field. The supported keywords for IPHDR_FIELD are:

    src
    dst
        Source or destination IP address, a four-byte value.

    tos
    dsfield
    precedence
        Type Of Service field, an eight-bit value.

    ihl Change the IP Header Length field, a four-bit value.

    protocol
        Next-layer Protocol field, an eight-bit value.

    nofrag
    firstfrag
    ce
    df
    mf
        Change IP header flags. Note that the value to pass to the set command is not just a bit value, but the full byte including the flags field. Though only the relevant bits of that value are respected, the rest ignored.

ip BEYOND_IPHDR_FIELD
    Supported only for non-extended layered op. It is passed to the kernel as offsets relative to the beginning of the IP header and assumes the IP header is of minimum size (20 bytes). The supported keywords for BEYOND_IPHDR_FIELD are:

    dport
    sport
        Destination or source port numbers, a 16-bit value. Indeed, IPv4 headers don't contain this information. Instead, this will set an offset which suits at least TCP and UDP if the IP header is of minimum size (20 bytes). If not, this will do unexpected things.

    icmp_type
    icmp_code
        Again, this allows one to change data past the actual IP header itself. It assumes an ICMP header is present immediately following the (minimal sized) IP header. If it is not or the latter is bigger than the minimum of 20 bytes, this will do unexpected things. These fields are eight-bit values.

ip EX_IPHDR_FIELD
    Supported only when ex is used. The supported keywords for EX_IPHDR_FIELD are:

    ttl

ip6 IP6HDR_FIELD
    The supported keywords for IP6HDR_FIELD are:

    src
    dst
    traffic_class
    flow_lbl
    payload_len
    nexthdr
    hoplimit

tcp TCPHDR_FIELD
    The supported keywords for TCPHDR_FIELD are:

    sport
    dport
        Source or destination TCP port number, a 16-bit value.

    flags

udp UDPHDR_FIELD
    The supported keywords for UDPHDR_FIELD are:

    sport
    dport
        Source or destination TCP port number, a 16-bit value.

clear
    Clear the addressed data (i.e., set it to zero).

invert
    Swap every bit in the addressed data.

set VAL
    Set the addressed data to a specific value. The size of VAL is defined by either one of the u32, u16 or u8 keywords in RAW_OP, or the size of the addressed header field in LAYERED_OP.

add VAL
    Add the addressed data by a specific value. The size of VAL is defined by the size of the addressed header field in EXTENDED_LAYERED_OP. This operation is supported only for extended layered op.

decrement
    Decrease the addressed data by one. This operation is supported only for ip ttl and ip6 hoplimit.

preserve
    Keep the addressed data as is.

retain RVAL
    This optional extra part of CMD_SPEC allows one to exclude bits from being changed. Supported only for 32 bits fields or smaller.

CONTROL
    The following keywords allow one to control how the tree of qdisc, classes, filters and actions is further traversed after this action.

    reclassify
        Restart with the first filter in the current list.

    pipe
        Continue with the next action attached to the same filter.

    drop
    shot
        Drop the packet.

    continue
        Continue classification with the next filter in line.

    pass
        Finish classification process and return to calling qdisc for further packet processing. This is the default.

EXAMPLES
Being able to edit packet data, one could do all kinds of things, such as e.g. implementing port redirection. Certainly not the most useful application, but as an example it should do: First, qdiscs need to be set up to attach filters to. For the receive path, a simple ingress qdisc will do, for transmit path a classful qdisc (HTB in this case) is necessary:
        tc qdisc replace dev eth0 root handle 1: htb
        tc qdisc add dev eth0 ingress handle ffff:
Finally, a filter with pedit action can be added for each direction. In this case, u32 is used matching on the port number to redirect from, while pedit then does the actual rewriting:
        tc filter add dev eth0 parent 1: u32 \
        	match ip dport 23 0xffff \
        	action pedit pedit munge ip dport set 22
        tc filter add dev eth0 parent ffff: u32 \
        	match ip sport 22 0xffff \
        	action pedit pedit munge ip sport set 23
        tc filter add dev eth0 parent ffff: u32 \
        	match ip sport 22 0xffff \
        	action pedit ex munge ip dst set 192.168.1.199
        tc filter add dev eth0 parent ffff: u32 \
        	match ip sport 22 0xffff \
        	action pedit ex munge ip6 dst set fe80::dacb:8aff:fec7:320e
        tc filter add dev eth0 parent ffff: u32 \
        	match ip sport 22 0xffff \
        	action pedit ex munge eth dst set 11:22:33:44:55:66
        tc filter add dev eth0 parent ffff: u32 \
        	match ip dport 23 0xffff \
        	action pedit ex munge tcp dport set 22
To rewrite just part of a field, use the retain directive. E.g. to overwrite the DSCP part of a dsfield with $DSCP, without touching ECN:
        tc filter add dev eth0 ingress flower ... \
        	action pedit ex munge ip dsfield set $((DSCP << 2)) retain 0xfc
And vice versa, to set ECN to e.g. 1 without impacting DSCP:
        tc filter add dev eth0 ingress flower ... \
        	action pedit ex munge ip dsfield set 1 retain 0x3

SEE ALSO
tc(8), tc-htb(8), tc-u32(8)